## PTL logo**Paterson Timber Limited**

140 Elliot Street, Glasgow   
0141 221 6445   
[**sales@paterson-timber.com**](mailto:sales@paterson-timber.com)  
Instagram: @patersontimber

www.paterson-timber.com

## ***STOCK SHEET – March 2024***

### **Hardwoods**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | 1” | 1 ¼ “ | 1 ½” | 2” | 2 ½” | 3” | 4” |
|  | 25.4mm | 31.8mm | 38.1mm | 50.8mm | 63.5mm | 76.2mm | 101.6mm |
| DARK RED MAJAU |  |  |  |  |  |  |  |
| DARK RED MERANTI |  |  |  |  |  |  |  |
| AMERICAN WHITE ASH |  |  |  |  |  |  |  |
| AMERICAN WHITE OAK |  |  |  |  |  |  |  |
| AMERICAN HARD WHITE MAPLE |  |  |  |  |  |  |  |
| AMERICAN RED CHERRY |  |  |  |  |  |  |  |
| PREMIUM GRADE WALNUT |  |  |  |  |  |  |  |
| AMERICAN RED OAK |  |  |  |  |  |  |  |
| AMERICAN TULIPWOOD |  |  |  |  |  |  | ✓ |
| PRIME GRADE EUROPEAN OAK |  |  |  |  |  |  |  |
| WANEY EDGE, PIPPY OAK |  |  |  |  |  |  |  |
| EUROPEAN STEAMED BEECH CND |  |  |  |  |  |  |  |
| EUCALYPTUS RED GRANDIS | ✓ |  |  |  |  |  |  |
| AFRICAN SAPELE |  | ✓ |  |  |  |  |  |
| AFRICAN SIPO / UTILE |  |  |  |  |  |  | ✓ |
| AFRICAN IROKO |  |  |  |  |  |  |  |
| AFRICAN FRAMIRE (IDIGBO) |  |  |  |  |  |  |  |
| AFRICAN AGBA |  |  |  |  |  |  |  |

The roof of a building

Description automatically generated A picture containing building, bench

Description automatically generated

**North American Stock** **Malaysian and African Stock**

**Softwoods**

**NORTH AMERICAN SOFTWOOD SET SIZES**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **150** | **280** | **300** |
| **CLEAR DOUGLAS FIR** |  |  |  |
| 38x |  |  |  |
| **SOUTHERN YELLOW PINE** |  |  |  |
| 25 x |  |  |  |
| 38 x |  |  |  |
| 50 x |  |  |  |
| **CLEAR WESTERN RED CEDAR** |  |  |  |
| 25 x |  |  |  |

**UNSORTED FINNISH RED PINE SAWN & BOARDS (PEFC Certified Stock)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **100** | **125** | **150** | **175** | **200** | **225** |
| **19 (Boards)** x |  |  |  |  |  |  |
| **25 (Boards)** x |  |  |  |  |  |  |
| **38 (4ex)** x |  |  |  |  |  |  |
| **50** x |  |  |  |  |  |  |
| **63**  x |  |  |  |  |  |  |
| **75** x |  |  |  |  |  |  |
| **100** x |  |  |  |  |  |  |

**A wooden table

Description automatically generated A picture containing container, building, wooden, floor

Description automatically generated**

**Finnish Red Pine Boards Western Red Cedar**

**SAWFALLING WHITE PINE STAIRWOOD SAWN (Certified Stock)**

38 x 275

**UNSORTED SIBERIAN LARCH KILN DRIED (Certified Stock)***Due to current sanctions once we run out of material we won’t be able to bring any more in*

50 x 200, 4.0 metre lengths

**Modified Products**

*Modified products enhance the properties of a timber with low durability outdoors to give it a greater lifetime and improve durability, similar to a slow grown hardwood.*

|  |  |  |
| --- | --- | --- |
| **A1 Grade Accoya** | **A2 Grade Accoya** | **Durawood Thermowood** |
| 25 x 200, 4.8 metres | 50 x 200, 4.8 metres | 26 x 360, 5.05 |
| 38 x 150, 4.8 metres | 63 x 200, 4.2 metres |  |
| 50 x 100, 2.4 metres | 75 x 200, 4.2 metres |  |
| 50 x 150, 4.8 metres |  |  |
| 63 x 125, 2.4 metres |  |  |
| 63 x 150, 4.8 / 2.4 metres |  |  |
| 75 x 150, 4.8 metres |  |  |

**Veneered Products**

**DECORATIVE VENEERED MDF BOARDS** (Other Veneered Boards can be manufactured to order)

V1S – Veneered 1 Side V2S – Veneered 2 Sides

3050 x 1220 = 10 x 4 2440 x 1220 = 8 x 4

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 3050 x 1220 | 2440 x 1220 | | |
|  | 19mm V2S A/B | 19mm V2S A/B | 13mm V2S A/B | 4mm V1S + Balancer |
| American Walnut |  |  |  |  |
| White Beech |  |  |  |  |
| Steamed Beech |  |  |  |  |
| Crown Cut White Ash |  |  |  |  |
| Cherry |  |  |  |  |
| Maple |  |  |  |  |
| Pine |  |  |  |  |
| Quarter Cut White Oak |  |  |  |  |
| Crown Cut White Oak |  |  |  |  |
| Baltic Pine (A/A) |  |  |  |  |
| Quarter Cut Sapele |  |  |  |  |
| Crown Cut Sapele |  |  |  |  |

*We also carry Crown Cut Oak in the following:*

|  |  |  |  |
| --- | --- | --- | --- |
|  | 2440 x 1220 | | |
|  | 26mm V2S A/B | 10mm V2S A/B | 6mm V2S A/B |
| Crown Cut White Oak |  |  |  |

**Pre-Glued Real Wood Edging Tape**

**22mm x 50 metre rolls only available:** Ash, Cherry, Maple, Pine, Beech, Steamed Beech, Sapele, Douglas Fir, Oak, Walnut

**50mm x 50 metre rolls available:** Walnut, Oak

**Decoflex Flexible Veneer**  
**0.6mm x 3050mm x 1240mm available**: Crown Cut Oak, Crown Cut Walnut, Crown Cut Ash

** A picture containing wall, indoor, brown, sitting

Description automatically generated**

**Veneered Walnut MDF White Oak Edging tape**

**Laminated Products**

**Clear Faced** **(C/F)** – Solid 10mm piece on top of each face

**2 Part** – Made up 2 sections with a mid-joint, colour matched for appearance   
**Edge glued (E/G)** – Different sections glued along the edge to give greater dimension size  
**Finger Jointed (F/J)** - complementary, interlocking sections put together to give greater stability after being glued. The finished look resembles ‘interlocking’ fingers

Our Laminated Products are detailed as **‘Thickness x Face’**

72x96 96x72  
FACE (F/J) FACE (F/J)

**Laminated**

**Laminated Window Sections**

**Laminated Red Pine KD Certified – available in 6.0m lengths**

**Finger Jointed – Available in 6.0m lengths**63 x 63, 63 x 75, 63 x 86, 63 x 96, 63 x 120, 72 x 60, 72 x 72, 72 x 86, 72 x 96, 72 x 145(J), 86 x 72, 96 x 63, 96 x 75, 96 x 96

**Laminated Eucalyptus Grandis KD Certified   
Finger Jointed – Available in 5.9m – 6.0m lengths**63 x 63, 63 x 86, 63 x 95, 63 x 200(J), 72 x 75, 72 x 86, 84 x 75, 96 x 63, 96 x 75, 96 x 96, 126 x 63

**Laminated Sapele KD –   
Finger Jointed - Available in 5.9 metre lengths**120 x 48A picture containing wooden, ground, building, table

Description automatically generated **F/J Laminated Red Pine KD F/J Laminated Eucalyptus Grandis KD**

**Laminated Stair Sections**

**Laminated European Oak KD Certified  
*Finger Jointed & Edge Glued*  
STRINGERS**  - 275 x 32 – Available in 4.8 metre lengths  ***Clear Faced***  
**NEWELS** - 90 x 90 – Available in 3.0m, 2.1m, 1.8m, 1.7m, 1.5m lengths  
**HANDRAIL** - 63 x 63 – Available in 4.8m  
A /B Grade (Supreme Colour Match) – A face has up to 3 joints, B face has 3 joints or more/  
B / B – more than 3 joints on each face

**BALUSTER/ SPINDLE SQUARES (Jointed)** - 41 x 41 – Available in 0.915m, 1.1m lengths

***Edge Glue only*  
Treads** 275 x 25, 275 x 32 – Available in 1.0m lengths

**A picture containing building, outdoor, floor, person

Description automatically generated**

**European Oak Handrails Clear Faced Laminated European Oak Newels**

**Laminated American White Oak  
*Edge Laminated and Colour Matched – Available in lengths ranging from 2.0m – 5.0m***

**2 piece** – 275 x 32

A close up of a wood surface

Description automatically generated with medium confidence

**Laminated Red Pine  
*Edge Glued and Shrink Wrapped* – *Has Sound Knots***  
**STRINGERS -** 270 x 33 (A/B Grade) – Available in 4.45m, 4.75m and 5.05m lengths

**STRINGERS -** 270 x 33 Bullnosed – Available in 3.0 metre lengths

***Finger Jointed, Edge Glued – Knot Free*STRINGERS -** 275 x 33 – Available in 6.0m lengths  
**STRINGERS -** 288 x 36 – Available in 6.0m lengths



**Left:** Shrink Wrapped Red Pine Stringers with sound knots compared to **Right:** Finger Jointed Red Pine Stringers (knot free)

**Laminated Door Sections**

**Laminated European Oak KD   
*Clear Faced* – Available in 2.5m, 2.1m, 1.1m, 0.9m lengths**

48 x 105, 48 x 120, 60 x 105, 60 x 120

**Laminated Red Pine KD Certified   
*Finger Jointed*** – Available in 6.0m lengths

120 x 48, 192 x 48, 192 x 60, 144 x 60, 120 x 60  
***Clear Faced Available* –** Available in 2.5m, 2.1m, 1.1m, 0.9m

48 x 105, 48 x 120, 60 x 105, 60 x 120

**Dark Red Meranti KD Certified**

***Clear Faced Laminated* -** Available in 2.5m, 2.1m48 x 120, 60 x 120

**Laminated Eucalyptus Grandis KD Certified**

***Finger Jointed - Available in long lengths***63 x 200, 125 x 63, 63 x 120

***Clear Faced Laminated***63 x 105, 63 x 120, 63 x 125

**C/F Laminated European Oak C/F Laminated Dark Red Meranti**

**A picture containing wooden, building, table, indoor

Description automatically generated A picture containing building, ground

Description automatically generated   
  
C/F Laminated Red Pine**

**A close up of a brick building

Description automatically generated**

***Other items may be available upon request***